Lag (ms)

Cochlear channel number

0 -10 -20 10 20

10 20 30 40 50 60 70 80 90

C. Box width doubled repeatedly. When box width exceeds half image width, left edge is shifted to fit box in image.