Lag (ms)

Cochlear channel number

0 -10 -20 10 20

10 20 30 40 50 60 70 80 90

B. Box height doubled repeatedly until box height is more than half SAI height