Lag (ms)

Cochlear channel number

0 -10 -20 10 20

10 20 30 40 50 60 70 80 90

A. Boxes tiled vertically overlapping by half height